Minutes meeting 01/02/16

-Beata and Tomasc presented the pedestal study, using the runs from the HV scan. The mean values seem correct but the rms was negative. They will investigate this point more carefully.

- Sacha proposed a simple approach to extract the signal: take the maximum of the signal where the time is in between the bin 9 and the bin 15. This should be our standard until new definition